Power Supply Parts List (Figure 3)

Resistors, if not marked otherwise, are metal film 0.6 W, 1% tolerance, MO = Metal Oxide 2 W, 2% tolerance, and MOX = Metal Oxide 4.5 W, 5% tolerance

Capacitors

C1,2 220 µF/450 V

C3 47 µF/100 V

Diode

D1 1 N 4007

Drive

Driver D-2075, 2 H/0.4 A, RDC <15 Ω

Ground

Gl1 GBU 4 J

Miscellaneous

1 pair fuse holder clips

fuse rating abaout 1.5 to 2 times AC current of transformer, slow blow

Circuit board, epoxy resin glasfiber reinforced, 70 µm copper cover, 90 mm × 110 mm, (board number –EE-309 A)

Relay

Rel1 Relay, 12 V, SPST, gold-plated contacts, 8 A

Resistors

R1,2 150 kΩ, MO

R3 47 kΩ