Power Supply Parts List (Figure 5)

Resistors, if not marked otherwise, are metal film 0.6 W, 1% tolerance, MO = Metal Oxide 2 W, 2% tolerance, and MOX = Metal Oxide 4.5 W, 5% tolerance

Capacitors

C5,7–12 100 µF/500 V

C6 100 µF/100 V

Diode

D1 1 N 4007

Drives

Dr1 D-2360, 2.3 H/0.6 A, RDC ≤ 30 Ω

Dr2 D-4060, 4 H/0.2 A, RDC ≤ 30 Ω

Fuses

F1,2 fuse, 0.63 A, slow blow

Grounds

Gl1,2 GBU 4 J

Miscellaneous

2 pairs fuse holder clips

Circuit board, epoxy resin glasfiber reinforced, 70 µm copper cover, 55 mm × 190 mm, (board number –EE-296 A)

Resistors

R1–4 150 KΩ, MO

R5 47 kΩ